nRF\_DFU

components\ble\ble\_services\ble\_dfu\ble\_dfu.c

components\ble\ble\_services\ble\_dfu\ble\_dfu\_bonded.c

components\ble\ble\_services\ble\_dfu\ble\_dfu\_unbonded.c

nRF\_BLE

components\ble\peer\_manager\gatt\_cache\_manager.c

components\ble\peer\_manager\gatts\_cache\_manager.c

components\ble\peer\_manager\id\_manager.c

components\ble\peer\_manager\peer\_data\_storage.c

components\ble\peer\_manager\peer\_database.c

components\ble\peer\_manager\peer\_id.c

components\ble\peer\_manager\peer\_manager.c

components\ble\peer\_manager\pm\_buffer.c

components\ble\peer\_manager\security\_dispatcher.c

components\ble\peer\_manager\security\_manager.c

nRF\_Libraries

components\libraries\fds\fds.c

components\libraries\crc16\crc16.c

components\libraries\fstorage\nrf\_fstorage.c

components\libraries\fstorage\nrf\_fstorage\_sd.c

nRF\_svc

components\libraries\bootloader\dfu\nrf\_dfu\_svci.c

nrfutil pkg generate --hw-version 52 --application-version 1 --application LML\_EEG.hex --sd-req 0xaf --key-file private.key LML\_EEG1.zip

..\..\..\..\..\..\integration\nrfx\legacy\nrf\_drv\_spi.c

..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx\_spi.c

..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx\_spim.c

..\..\..\..\..\..\modules\nrfx\drivers\src\nrfx\_ppi.c

..\..\..\..\..\..\integration\nrfx\legacy\nrf\_drv\_ppi.c

BOARD\_PCA10040 CONFIG\_GPIO\_AS\_PINRESET FLOAT\_ABI\_HARD NRF52 NRF52832\_XXAA NRF52\_PAN\_74 NRF\_SD\_BLE\_API\_VERSION=6 S132 SOFTDEVICE\_PRESENT SWI\_DISABLE0 \_\_HEAP\_SIZE=8192 \_\_STACK\_SIZE=8192 DEBUG NRF\_DFU\_TRANSPORT\_BLE=1 BL\_SETTINGS\_ACCESS\_ONLY

BOARD\_PCA10040 CONFIG\_GPIO\_AS\_PINRESET FLOAT\_ABI\_HARD NRF52 NRF52832\_XXAA NRF52\_PAN\_74 NRF\_SD\_BLE\_API\_VERSION=6 S132 SOFTDEVICE\_PRESENT SWI\_DISABLE0 \_\_HEAP\_SIZE=8192 \_\_STACK\_SIZE=8192 DEBUG NRF\_DFU\_TRANSPORT\_BLE=1 BL\_SETTINGS\_ACCESS\_ONLY